,Model##Other##,Series##Other##,Description##Other##,Shipping Weight##Other##,Product Page URL##Other##,Product Documentation Link##Other##,Catalog Number##Other##,Photometric Web File##Other##,Ballast Type##Other##,Width##Length##Inches,Length##Length##Inches,Height##Length##Inches,Has U Bulb##Other##,Has Straight Bulb##Other##,Has Biaxial Bulb##Other##,CTRL Reflector 1 Left Inset##Length##Inches,CTRL Reflector 2 Left Inset##Length##Inches,CTRL Reflector 1 Elevation Inset##Length##Inches  ,CTRL Reflector 2 Elevation Inset##Length##Inches,CTRL Lamp 1 Height Inset##Length##Inches,CTRL Lamp 2 Height Inset##Length##Inches,CTRL Lamp 3 Height Inset##Length##Inches,CTRL Lamp 4 Height Inset##Length##Inches,CTRL Light Source 1 Offset##Length##Inches,CTRL Light Source 2 Offset##Length##Inches,CTRL Light Source 3 Offset##Length##Inches,CTRL Light Source 4 Offset##Length##Inches,CTRL Lamp 1 Left Inset##Length##Inches,CTRL Lamp 2 Distance From 1##Length##Inches,CTRL Lamp 3 Distance From 2##Length##Inches,CTRL Lamp 4 Distance From 3##Length##Inches,CTRL Bulb Diameter##Length##Inches,CTRL Bulb U Separation Distance##Length##Inches,Lamp Quantity##Other##,Supply Voltage##Electrical_Potential##Volts,Voltage##Other##,Total Input Wattage##Other##,Efficiency##Other##,Lamp##Other##,Wattage##electrical_wattage##watts,Wattage Comments##Other##,CTRL End Cap Length Distance##Length##Inches,Shield Type##Other##,Housing Type##Other##,End Cap Type##Other##,Reflector Type##Other##,Efficacy##electrical_efficacy##lumens_per_watt
4'_Commercial_Grade_Wrap_WN-3Lamp-28W-T5-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081677_WN_3L_T5.pdf,WN-328T5,WN328T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,120,120,97,94.50%,T5,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,74
4'_Commercial_Grade_Wrap_WN-3Lamp-28W-T5-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081677_WN_3L_T5.pdf,WN-328T5,WN328T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,227,227,97,94.50%,T5,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,74
4'_Commercial_Grade_Wrap_WN-3Lamp-28W-T5-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081677_WN_3L_T5.pdf,WN-328T5,WN328T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,0,0,97,94.50%,T5,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,74
4'_Commercial_Grade_Wrap_WN-3Lamp-54W-T5HO-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081677_WN_3L_T5.pdf,WN-354T5,WN328T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,120,120,185,94.50%,T5HO,54,54,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,74
4'_Commercial_Grade_Wrap_WN-3Lamp-54W-T5HO-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081677_WN_3L_T5.pdf,WN-324T5,WN328T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,227,227,185,94.50%,T5HO,54,54,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,74
4'_Commercial_Grade_Wrap_WN-3Lamp-54W-T5HO-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081677_WN_3L_T5.pdf,WN-328T5,WN328T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,0,0,185,94.50%,T5HO,54,54,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,74
4'_Commercial_Grade_Wrap_WN-3Lamp-28W-T8-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081639_WN_3L_T8.pdf,WN-328T8A,WN328T5A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,120,120,67,83.50%,T8,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-3Lamp-28W-T8-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081639_WN_3L_T8.pdf,WN-328T8A,WN328T5A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,227,227,67,83.50%,T8,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-3Lamp-28W-T8-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081639_WN_3L_T8.pdf,WN-328T8A,WN328T5A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,0,0,67,83.50%,T8,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-3Lamp-32W-T8-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081639_WN_3L_T8.pdf,WN-332A,WN332A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,120,120,80,83.50%,T8,32,32,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-3Lamp-32W-T8-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081639_WN_3L_T8.pdf,WN-332A,WN332A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,227,227,80,83.50%,T8,32,32,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-3Lamp-32W-T8-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081639_WN_3L_T8.pdf,WN-332A,WN332A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,3.75,3.75,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,4.625,4.5,0,1,2,3,0,0,80,83.50%,T8,32,32,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-4Lamp-28W-T5-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,8,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081675_WN_4L_T5.pdf,WN-428T5,WN428T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,120,120,131,87.90%,T5,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,68
4'_Commercial_Grade_Wrap_WN-4Lamp-28W-T5-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,8,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081675_WN_4L_T5.pdf,WN-428T5,WN428T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,227,227,131,87.90%,T5,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,68
4'_Commercial_Grade_Wrap_WN-4Lamp-28W-T5-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,8,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081675_WN_4L_T5.pdf,WN-428T5,WN428T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,0,0,131,87.90%,T5,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,68
4'_Commercial_Grade_Wrap_WN-4Lamp-54W-T5HO-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,8,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081675_WN_4L_T5.pdf,WN-454T5,WN454T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,120,120,226,87.90%,T5HO,54,54,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,68
4'_Commercial_Grade_Wrap_WN-4Lamp-54W-T5HO-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,8,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081675_WN_4L_T5.pdf,WN-454T5,WN454T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,227,227,226,87.90%,T5HO,54,54,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,68
4'_Commercial_Grade_Wrap_WN-4Lamp-54W-T5HO-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T5 LAMPS Commercial Wrap,8,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081675_WN_4L_T5.pdf,WN-454T5,WN454T5A.ies,T5/T5HO Linear Electronic Program Rapid Start,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,0,0,226,87.90%,T5HO,54,54,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,68
4'_Commercial_Grade_Wrap_WN-4Lamp-28W-T8-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081640_WN432_4L.pdf,WN-428T8A,WN428T5A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,120,120,93,79.10%,T8,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-4Lamp-28W-T8-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081640_WN432_4L.pdf,WN-428T8A,WN428T5A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,227,227,93,79.10%,T8,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-4Lamp-28W-T8-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081640_WN432_4L.pdf,WN-428T8A,WN428T5A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,0,0,93,79.10%,T8,28,28,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-4Lamp-32W-T8-120V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081640_WN432_4L.pdf,WN-432A,WN432A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,120,120,102,79.10%,T8,32,32,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-4Lamp-32W-T8-227V,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081640_WN432_4L.pdf,WN-432A,WN432A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,227,227,102,79.10%,T8,32,32,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
4'_Commercial_Grade_Wrap_WN-4Lamp-32W-T8-UNV,4' Commercial Grade Wrap WN,Series WN,4' SURFACE T8 LAMPS Commercial Wrap,12,http://www.cooperindustries.com/content/public/en/lighting/products/indoor_ceiling_wall_mount_lighting/ceiling_mount/_135329.html,http://www.cooperindustries.com/content/dam/public/lighting/products/documents/Metalux/spec_sheets/081640_WN432_4L.pdf,WN-432A,WN432A.ies,T8 Electronic Instant Start. ,12,48,2.5,0,1,0,6,6,0.5,0.5,1.5,1.5,1.5,1.5,2.5,1,1,1,1.5,2.1875,4.625,2.1875,1,2,4,0,0,102,79.10%,T8,32,32,48,Shield 2 - 3_Sides-Angled : 1' x 4',Housing 3 - Angled : 1' x 4',"End Cap 2 - Angled : 12""",Reflector 2 - Triangular : Flat Top,84
